Pulsed Nano- and picosecond Discharge Development in Liquids

A. Starikovskiy

Princeton University, Princeton, U.S.A., astariko@princeton.edu

Three possible mechanisms for the propagation of discharge in liquids play a different role depending on the pulse duration. The first case takes place when a "long" (microsecond) electric pulse applied in a non-conducting fluid: as a result of electrostatic repulsion, the formation of low density channels occurs. Consequently, the discharge propagates through the low-density regions [1]. In the second case, under an "intermediate" (nanosecond) electric pulse conditions, the electrostatic forces support the expansion of nanoscale voids behind the front of the ionization wave; in the wave front the extreme electric field provides a strong negative pressure in the dielectric fluid due to the presence of electrostriction forces, forming the initial micro-voids in the continuous medium [2, 3]. Finally, in the third case, when a "short" (picosecond) electric pulse is utilized, the regions of reduced density cannot form because of the extremely short duration of the applied electric pulse. Ionization in the liquid phase occurs as a result of direct electron impact without undergoing a phase transition, occurring due to the acceleration of electrons by an external electric field comparable to the intra-molecular fields. In this case, the discharge propagates with a velocity comparable to the local speed of light [4, 5].

The differences in the nanosecond discharge development in liquid dielectrics with different dielectric permittivity coefficients show a significant decrease in the breakdown threshold for discharge in water in comparison to that of hexane, which may be explained by the formation of micro-discontinuities in the media during the electrostriction compression/rarefaction stage, specifically in liquids with high dielectric permittivity coefficients. In two other cases – for “long” microsecond and “short” picosecond pulses – the dielectric permittivity of the liquid plays only a minor role for the discharge formation.

References

1. P. Bruggeman and C. Leys. Non-thermal plasmas in and in contact with liquids. J. Phys. D: Appl. Phys. 42 (2009) 053001 (28pp)
2. A. Starikovskiy. Pulsed nanosecond discharge development in liquids with various dielectric permittivity constants. Plasma Sources Sci. Technol. 22 (2013) 012001 (5pp)
3. M. Shneider, M. Pekker and A. Fridman. Theoretical Study of the Initial Stage of Sub-nanosecond Pulsed Breakdown in Liquid Dielectrics. IEEE Transactions on Dielectrics and Electrical Insulation. Vol. 19, No. 5; October 2012. 1579.
4. A. Starikovskiy, Y. Yang, Y. Cho, A. Fridman. Nonequilibrium Plasma in Liquid Water - Dynamics of Generation and Quenching. Plasma Sources Sci. Technol. 20 (2011) 024003.
5. A. Starikovskiy, Y. Yang, Y.. Cho, A. Fridman. Nonequilibrium liquid plasma generation. IEEE Transactions on Plasma Science. V 39. N 11. 2011. pp. 2668-2669.