GENERATION OF SOFT X-RAY RADIATION IN THE INTERACTION OF A POWERFUL PLASMA FLOW WITH A GAS AND SOLID-STATE TARGETS IN A MAGNETIC FIELD [[1]](#footnote-1)\*)

DOI: 10.34854/ICPAF.2022.49.1.042

1,2Toporkov D.A., 1,5Burmistrov D.A., 1Gavrilov V.V., 1Zhitlukhin A.M., 1Kostyushin V.A., 1,2Lidzhigoryaev S.D., 1,4Pushina A.V., 3,4Pikuz S.A., 3,4Ryazantsev S.N., 3,4Skobelev I.Yu.

1SSC RF TRINITI, toporkov@triniti.ru
2NIU Moscow Institute of Physics and Technology
3Joint Institute for High Temperatures of the Russian Academy of Sciences
4NIU Moscow Engineering Physics Institute
5NIU Moscow Power Engineering Institute

The report presents the results of a study of a powerful hydrogen plasma flow with a pulsed nitrogen jet and a tungsten target. Experimental data can be useful both from a fundamental point of view and in solving a number of applied problems (for example, for developing the concept of the ITER dissipative divertor and laboratory modeling of stellar jets penetrating into a galactic gas).

A plasma flow with a speed of (4÷6)×107 cm∙s-1 and an energy content of up to 40 kJ was created by a pulsed electrodynamic accelerator MKT (SRC RF TRINITI). The density of the plasma flow was (2÷4) × 1015 cm-3. The plasma flow was transported in a longitudinal magnetic field with an induction of 1÷2 T and interacted with a plane supersonic nitrogen jet, behind which a tungsten target was located at a distance of 1÷3 cm. The maximum density in the gas jet reached 1017 cm-3 with a jet thickness of ≈ 5 cm and a width of ≈ 15 cm.

SXR images of the interaction region of the plasma with the gas and the target, as well as the radiation spectra of the target plasma in the range of 1÷30 nm were recorded using a multi-frame MCP camera. For the absolute power of plasma SXR radiation, FDUK-8UVS photodiodes were used. The electron temperature of the plasma was determined by comparing the experimental spectra with the spectra obtained as a result of detailed kinetic calculations of the line plasma radiation, and was in the range 40÷50 eV at distances ≥ 4 mm from the target surface. In this case, the characteristic spectra of tungsten, observed in the absence of a nitrogen jet at a distance of up to 5÷6 cm from the target, were much smaller in the presence of gas in front of the tungsten surface already at a distance of ≈1cm.

This work was carried out with financial support within the framework of scientific projects of the Russian Foundation for Basic Research No. 18-29-21013 and No. 20-21-00153.

1. \*) [abstracts of this report in Russian](http://www.fpl.gpi.ru/Zvenigorod/XLIX/Mu/ru/CI-Toporkov.docx) [↑](#footnote-ref-1)