Plain and Brominated low-density steady parylene as Diagnostic and construction target layer for the research experiments in the context of icf

I.V. Akimova1, A.A. Akynets1, L.A. Borisenko2, A.I. Gromov1, A.S. Orekhov1, and N.G. Borisenko1

1Lebedev Physical Institute, Russian Academy of Sciences, Moscow, Russia
 ngbor@sci.lebedev.ru
2Moscow State University, Moscow, Russia, borisenko.lidiya@physics.msu.ru

Parylene is a high steady plastic (C8H8) generally used as a micron protective layer of internal surfaces in microcircuits, and may contain Br: brominated parylene (C8H7Br) [1].

In such a form Br enters the plastic formula and may be used as a diagnostic agent in the reaction 79Br(n,2n)78Br in the ICF targets [2].

In one of the experiments on the preparation of thin wall billets for cylindrical targets we succeeded in producing a porous low density (1/5–1/10 of the solid C8H7Br) material, and this is of interest for the experimental targets [3, 4].

Low density brominated parylene possesses sufficient strength and flexibility, it is thermostable and can be used as a construction material for the target layers. Low density layers in the ICF targets are promising, and have a number of advantages [5].

In the course of the work the authors have succeeded in overcoming the problems associated with complex preparation procedures and the conduction of the reaction in a limited vacuum volume with the sublimation temperature 850oC, the deposition at -1400C, and further long pumping.

The work was supported in part by the Russian Foundation for Basic Research (grants № 15-52-451and 15-02-08113a).

References

1. Bieg K.W. Summary Abstract: Metal loaded poly-p-xylylene // Journal of Vacuum Science and Technology.1981.A18(3). P. 1231-1232.
2. Gromov A.I., Merkuliev Yu.A**.** Diagnostic Laser Targets // Laser Thermonuclear Targets and Superdurable Microballoons. Edited by A.I. Isakov, Nova Scienceг Publishers, Inc,1996, 57-72.
3. A.I. Gromov, N.G. Borisenko, S.Y. Gus'kov, Yu.A. Merkuliev, et al. [Fabrication and monitoring of advanced low-density media for ICF targets](http://wos.isiknowledge.com/?SID=B6gE7jPGnia2k66Nm@a&Func=Abstract&doc=1/7). // Laser and particle Beams, 1999, Vol. 17, No 4, pp. 661-670.
4. Belyaev V.S., Matafonov A.P., Vinogradov V.I., Garanin S.G., Borisenko N.G., Chekmarev A.M., Demchenko N.N., Gromov A.I., Guskov S.Yu., Khalenkov A.M., Merkuliev Yu.A., Rozanov V.B., Andrianov V.P., Ignat’ev G.N., Markushkin Yu.E, and Pimenov V.G.Composition, density and structure dependent neutron yields from deuterated targets in high-intensity laser shot// J.Phys.IV Franс,v.133, p.507-509. 2006.
5. Spherical laser targets for projects of the XXI century..А.А.Акunets, А.А Аleksandrova, L.А. Borisenko et al. XLII International Zvenigorod Conference on Plasma Physics and Controlled Fusion. 2015. Book of Abstracts, p.147.